1 - Launch MCID_PAL.ELF or MCID_NTSC.ELF depending on your ps2.

2 - Put mcid.bin in ID Patch folder. 

3 - Run the batch and follow instructions.

4 - You will found your patched memcard image in ID Patch folder.
    Fell free to modify it with Mymc

5 - Run HdProject - McFlasher and flash your memcard with the memcard image.
    Let port and slot options to 0, ECC skip : NO 
    DATEL never formatted option is intended for ecc emulation cards (Datels never reformatted have it), 
    so don't touch it unless your card is a Datel that you have never formatted yourself.
    In case something goes bad for your card, armax evo will revive it.

6 - Copy the BOOT-FREE-OSD to your usb stick root(optional).

7 - Insert memcard and usb stick(optional) and boot.

8 - On your memcard you will see a BOOT-FREE-OSD folder with an ELF in it(Ule).
    You can eventually replace it.  
